

**A picture containing blue

Description automatically generatedA picture containing blue

Description automatically generated**MEDIA CONTACTS

Wayne Hart

(714) 522-8088 x4410

[whart@makitausa.com](mailto:whart@makitausa.com)

Consumer Inquiries:

(800) 4-MAKITA

makitatools.com

@makitatools

**FOR IMMEDIATE RELEASE**

*Makita has expanded its dust extraction system with two new cordless HEPA dry vacuums available in 2.1 gallon capacity (XCV21PTX, left), and 4 gallon capacity (XCV24ZX, right). Both are powered by two 18V LXT batteries and an efficient 36V brushless motor that combines cleaning performance with cordless convenience.*

**MAKITA EXPANDS DUST EXTRACTION SYSTEM WITH TWO NEW HEPA DRY VACUUMS**

**New 2.1- and 4-gallon models give contractors more options for dust extraction and cleanups**

**February 18, 2022, La Mirada, CA** – Makita U.S.A., Inc., manufacturer of high-quality professional tools and accessories, has expanded its dust extraction system with two new HEPA dry vacuums. Both models are powered by two 18V LXT® batteries and an efficient 36V brushless motor, giving contractors two more cordless options for job site dust extraction and cleanups.

The new models include the following:

* **XCV21PTX** – 36V (18V X2) LXT® Brushless 2.1 Gallon HEPA Filter Dry Dust Extractor Kit (Also available as tool only, XCV21ZX)
* **XCV24ZX** - 36V (18V X2) LXT® Brushless 4 Gallon HEPA Filter Dry Dust Extractor, Tool Only

“There is more awareness of the importance of dust extraction, and more demand for the convenience of cordless vacuums,” said Wayne Hart, sr. communications manager, Makita U.S.A., Inc. “These two new LXT HEPA dry vacuums combine performance and capacity with the convenience of cordless – and they’re powered by the same fast-charging 18-volt batteries that run over 275 LXT products.”

**Long Run Time, HEPA Filter, and More**

Both the 2.1-gallon and 4-gallon Dust Extractors deliver up to 80 minutes of continuous runtime when using two 18V LXT® 5.0Ah batteries. The powerful Makita-built brushless motors deliver 74 CFM and 44" of water lift for efficient cleaning. Both the 2.1- and the 4-gallon dust extractors feature a three-stage HEPA filter that captures 99.97% of particulates .3 microns and larger.

**Lower Noise**

The motor chamber is constructed with sound-absorbing materials, emitting only 64dB(A) on the high setting. The dust extractors come equipped with an anti-static hose (1” x 11’) and three adaptor cuffs in 22, 24, and 38 mm that fit 1” hoses for added versatility. A removable storage box holds attachments and batteries.

**Expanding Dust Extraction System**

The new dust extractors are part of Makita’s expanding dust extraction system which includes canister and backpack vacuums, as well as a comprehensive range of attachments for concrete applications, woodworking, and more. Contractors seeking a system compliant with the OSHA Silica Standard Rule 29 CFR 1926.1153 can use the Makita website to quickly search by application, model number, and more. Find an ideal solution at [www.makitatools.com/buildyoursystem](http://www.makitatools.com/buildyoursystem)

**18V LXT® System**

The LXT® System, the world’s largest cordless tool system powered by 18V lithium-ion slide-style batteries, takes a user from power tools to outdoor power equipment to get the job done. Makita’s purpose-built motors, battery technology, and enhanced communications work together to deliver unmatched power, speed and run time. With solutions for every trade, users get maximum performance and efficiency with the LXT® System.

**Specifications**

|  |  |  |  |
| --- | --- | --- | --- |
| **Model Number** | **XCV21PTX Kit** | **XCV21ZX (Tool only)** | **XCV24ZX (Tool Only)** |
| **Name** | 36V (18V X2) LXT® Brushless 2.1 Gallon HEPA Filter Dry Dust Extractor Kit | 36V (18V X2) LXT® Brushless 2.1 Gallon HEPA Filter Dry Dust Extractor (Tool Only) | 36V (18V X2) LXT® Brushless 4 Gallon HEPA Filter Dry Dust Extractor (Tool Only) |
| **Battery Type** | 2X 18V LXT® Lithium-Ion | 2X 18V LXT® Lithium-Ion | 2X 18V LXT® Lithium-Ion |
| **Container Size (gal)** | 2.1 | 2.1 | 4 |
| **Airflow** | 74 CFM | 74 CFM | 74 CFM |
| **Static Water Lift** | 44" | 44" | 44" |
| **Continuous Use (high setting with two 18V LXT 5.0Ah batteries** | 80 min. | 80 min. | 80 min. |
| **HEPA Filters Available** | Yes | Yes | Yes |
| **AWS** | Yes | Yes | Yes |
| **Working Sound Level** | 64 dB(A) | 64 dB(A) | 64 dB(A) |
| **Net Weight (w/batteries)** | 16.8 lbs. | 16.8 lbs. | 17.2 lbs. |
| **Power Type** | Cordless | Cordless | Cordless |
| **Includes** | (2) 18V LXT® Lithium-Ion 5.0Ah batteries, dual port rapid charger, anti-static hose, main HEPA filter, damper, pre-filter, and three adapters | Anti-static hose, main HEPA filter, damper, pre-filter, and three adapters (battery and charger not included) | Anti-static hose, main HEPA filter, damper, pre-filter, and three adapters (battery and charger not included) |

**About Makita**

Makita is a worldwide manufacturer of industrial power tools, power equipment, pneumatics, and cleaning solutions that offer a wide range of industrial accessories. Makita U.S.A., Inc. is located in La Mirada, California, and operates an extensive distribution network throughout the U.S.A. With over 50 years in the United States and over 100 years worldwide, Makita utilizes experience and expertise to manufacture best-in-class solutions. For more information about Makita U.S.A. call (800)4-MAKITA or visit makitatools.com. Find Makita on Instagram, YouTube, Facebook, and Twitter @makitatools

-###-